**PRODUCT SPECIFICATION – SECTION 09510 – ACOUSTICAL CEILING PANELS
ConceptZtm Wool Stone Base** **: [23¾” x 23¾”] x [5/8”] acoustical ceiling panels as specified and indicated on drawings**

**2.1 MANUFACTURER**

1. Bluffview Development Group LLC: Aspens Design Legacy
2. Address: La Crosse, WI 54603
3. Phone Number: +1 (608) 518 6085
4. Website:[www.interiorsystems.com](http://www.interiorsystems.com)
5. Email: customercare@bluffviewgroup.com

 **2.2 ACOUSTIC CEILING UNITS**

A. Acoustical Ceiling Panel (ACP) - [Type ACP-1]

* + 1. Name: Digitally Printed Acoustical Ceiling Panels
		2. Physical Characteristics
			1. Pattern: Felt Digitally applied color: Grey,Beige, custom colors
			2. Size: 23.75’’x 23.75’’
			3. Thickness: 0.63’’
			4. Edge: Square Edge, Lay-in
			5. Finished Surface: Fine surface
			6. Finished Surface Color: Digitally Printed 4C UV Coating
			7. Core Composition: Stone Wool
			8. Recycled Content: 84%
		3. Performance Criteria
			- 1. Noise Reduction Coefficient (NRC): 0.75 (Base Tile)
				2. Ceiling Attenuation Class (CAC): 23
				3. Flame Spread Classification: Class A Non-combustible

