
**PRODUCT SPECIFICATION – SECTION 09510 – ACOUSTICAL CEILING PANELS  
ConceptZtm Wool Stone Base** **: [23¾” x 23¾”] x [5/8”] acoustical ceiling panels as specified and indicated on drawings**

**2.1 MANUFACTURER**

1. Bluffview Development Group LLC: Aspens Design Legacy
2. Address: La Crosse, WI 54603
3. Phone Number: +1 (608) 518 6085
4. Website:[www.interiorsystems.com](http://www.interiorsystems.com)
5. Email: [customer](mailto:ceilings@interiorsystems.com)care@bluffviewgroup.com

**2.2 ACOUSTIC CEILING UNITS**

A. Acoustical Ceiling Panel (ACP) - [Type ACP-1]

* + 1. Name: Digitally Printed Acoustical Ceiling Panels
    2. Physical Characteristics
       1. Pattern: Felt Digitally applied color: Grey,Beige, custom colors
       2. Size: 23.75’’x 23.75’’
       3. Thickness: 0.63’’
       4. Edge: Square Edge, Lay-in
       5. Finished Surface: Fine surface
       6. Finished Surface Color: Digitally Printed 4C UV Coating
       7. Core Composition: Stone Wool
       8. Recycled Content: 84%
    3. Performance Criteria
       - 1. Noise Reduction Coefficient (NRC): 0.75 (Base Tile)
         2. Ceiling Attenuation Class (CAC): 23
         3. Flame Spread Classification: Class A Non-combustible

